|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| * **Cristo Blocks**   **Mfrs. Of High Quality Cement Concrete Products** | | | | | **CONTACT:**  **9282225225**  **9282172052** | |
| **SL** | **IMAGE** | **NAME** | **Description** | **USAGE** | | **HSN CODE TAX RATE** |
| 1 |  | **8” CONCRETE BLOCK – SOLID**  **16” X 8” X 8”**  **(400 X 200 X 200MM)** | **High Density 40 tonnes loading capacity (comparable: 20 tonnes)** | All kind of masonry work | | 6810  18% |
| 2 |  | **6” CONCRETE BLOCK – SOLID**  **16” X 6” X 8”**  **400 X 150 X 200MM)** | **High Density 30 tonnes loading capacity (comparable: 15 tonnes)** | All kind of masonry work | | 6810  18% |
| 3 |  | **4” CONCRETE BLOCK – SOLID**  **16” X 4” X 8”**  **(400 X 100 X 200MM)** | **High Density 20 tonnes loading capacity (comparable: 10 tonnes)** | All kind of masonry work | | 6810  18% |
| 4 |  | **6” CONCRETE BLOCK – HOLLOW 2 - HOLES 12” X6” X 8”**  **(300 X 138 X 200MM)** | **Holes for TMT Bar and or Concrete** | All kind of masonry work | | 6810  18% |
| 5 |  | **6” CONCRETE BLOCK – HOLLOW**  **3 - HOLES**  **16” X 6” X 8”**  **(400 X 150 X 200MM)** | **Holes for TMT Bar and or Concrete** | All kind of masonry work | | 6810  18% |
| 6 |  | **HALF BLOCK 6”**  **CONCRETE BLOCK – SOLID**  **8” X6” X 8”**  **(200 X 150 X 200MM)** | **High Density 30 tonnes loading capacity (comparable: 15 tonnes)** | All kind of masonry work | | 6810  18% |

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Cristo Blocks**  **Mfrs. Of High Quality Cement Concrete Products** | | | | | **CONTACT:**  **9282225225**  **9282172052** | |
| **SL** | **IMAGE** | **NAME** | **Description** | **USAGE** | | **HSN CODE TAX RATE** |
| 7 |  | **BLOCK 8"X8"X8"**  **COLUMN BLOCK 1-HOLE** | **8"X8"X8" (200X200X200MM)** | Used for 4” com- pound wall | | 6810  18% |
| 8 |  | **BLOCK 10"X10"X8" COLUMN BLOCK**  **1-HOLE** | **10"X10"X8" (250X250X200MM)** | Used for 8” com- pound wall | | 6810  18% |
| 9 |  | **BLOCK 12"X12"X8" COLUMN BLOCK**  **1 HOLE** | **12"X12"X8" (300X300X200MM)** | Gate pillar 20’ span | | 6810  18% |
| 10 |  | **BLOCK 15"X8"X8"**  **COLUMN BLOCK 1-HOLE** | **15"X8"X8" (380X200X200MM)** | Used for up to 15 width | | 6810  18% |
| 11 |  | **BLOCK 18"X8"X8"**  **COLUMN BLOCK 1-HOLE** | **18"X8"X8" (450X200X200MM)** | Used for up to 18’ width | | 6810  18% |
| 12 |  | **BEAM**  **BEAM 111”X4”X8” WITH 4”X6” SLOT\*** | **For Blinth Beam and Lintel Beam** | Used as beam | | 6810  18% |